kea_cfg_opt15

Example of configuration for option 15 (dhcp6_poolname_opt=1) for Kea DHCPv6:

# Class Description "client-classes": [ { # opt15 User-Class "name": "ppp_userclass_ip6_pool", "test": "substring( option[15].hex, 2, 100 ) == 'ppp_userclass_ip6_pool'", # In option-data you can set options common to this class "option-data": [ { "name": "dns-servers", "space": "dhcp6", "data": "2001:db8:2::dead:cafe, 2001:db8:2::cafe:dead" } ] }, # Description of other classes # ... ] # end of client-classes # Setting pools "shared-networks": [ { "name": "MyNetworks", # The pools are accessed on behalf of the relay "relay": { "ip-addresses": ["2001::1"] }, "subnet6": [ { "client-class": "ppp_userclass_ip6_pool", "subnet": "2a02:400:1::/48", # IMPORTANT! Only a PD prefix with a length one less than the value of the # of the ipv6_subnetmask parameter in fastdpi.conf (default value is 64). # SSG itself splits this prefix into 2 ipv6_subnetmask lengths: the younger one # /64 subnet is given to the client, the older one is under the client prefix "pd-pools": [ { "prefix": "2a02:400:1::", "prefix-len":48, "delegated-len": 63 } ] } # description of other pools # ... ] # end of subnet6 ] # end of shared-networks