DHCP (local DHCP server for BRAS)

The component is activated in a scenario with a local DHCP server. We recommend using Kea DHCP server.

It is also possible to use SSG in:

DHCP-relay — redirect requests to a specific server

DHCP RADIUS proxy mode — information about the settings is transmitted in RADIUS responses, and SSG acts as a DHCP server.

DHCP Dual Proxy — in this mode, fastDPI operates as a single authorization point, requesting all parameters from the RADIUS server via fastPCRF in a single request.