DPI Configuration

Export Configuration

The DPI platform version must be at least 8.1!

IPFIX export is configured in the fastdpi.conf file on the DPI.

netflow=8
netflow_dev=em1
netflow_timeout=10
netflow_full_collector_type=2
netflow_full_port_swap=0
netflow_full_collector=YOUR_QOESTOR_IP:1500
ipfix_dev=em1
ipfix_tcp_collectors=YOUR_QOESTOR_IP:1501

A fastDPI restart is required for the changes to take effect.

The netflow parameter is a bitmask and can have multiple values. See more in section Configuring service.

Configuration in DPIUI2

The DPIUI2 version must be at least 2.1.0!

Go to the SSG control → Configuration section.

Navigate to the tab "Collection and analysis of statistics on protocols and directions" and apply the following settings:

Set the neflow parameter to "Export full session statistics"

Set the netflow_full_collector_type parameter to "Export ipfix to tcp header"

Enter the socket of the fullflow receiver in the netflow_full_collector parameter

Leave the netflow_full_port_swap parameter empty or set it to "Preserve original port numbers".

Navigate to the "PCAP Recording, IPFIX Export (Clickstream and metadata: SIP, FTP)" tab

Enter the clickstream receiver socket in the ipfix_tcp_collectors parameter.

Save the configuration

Restart the DPI

Assigning a DPI Number

Go to the Administrator → Equipment.

For each device, enter the Id on IPFIX collector.

Configuring DPIUI2 Connection to QoE Stor

To view QoE reports, you need to configure the connection between DPIUI2 and QoE Stor.
See more in the section Connecting to QoE Stor Configuration