IPFIX export configuration from SSG to QoE

Configuration in GUI

Export configuration

IPFIX export is configured in the fastdpi.conf file on the DPI.
Example of minimal recommended export settings:

netflow=8
netflow_dev=em1
netflow_timeout=10
netflow_full_collector_type=2
netflow_full_port_swap=0
netflow_full_collector=YOUR_QOESTOR_IP:1500
ipfix_dev=em1
ipfix_tcp_collectors=YOUR_QOESTOR_IP:1501

Additionally, you can configure export of NAT flows, DNS, GTP and RADIUS.
QoE must have receivers configured for all streams.

To apply the changes, fastDPI must be restarted.

The netflow parameter is a bitmask and can have several different values. See more in Set up NetFlow export by protocols, directions and billing.